Power Down

Start Up

Stand-by

TX Mode

RX Mode

TX Setting

RX Setting

PWR\_UP=0

PWR\_UP=0

PWR\_UP=0

PWR\_UP=1

CE=0

CE=1

CE=1

CE=1

CE=1

CE=1

CE=1

TIMEOUT != 0